BHEL | Phone 586100 Fax 0755-500023 | BHARAT HEAVY ELECTRICALS Ltd. (BHOPAL) | ENQUIRY | Enquiry | Total Items
No E3183111 | Date 12-08-2008 | . 3
Revision | Due Date of quotation | Vendor Code | Indent No | Supply Condition of Material
Code | No. | Date | IN WELL PACKED CONDITION TO AVOID TRANSIT DAMAGE.
1 | 0 |  | 20-09-2008 | SUPP_CODE |
To : enqs_supp_name enqs_supp_add1 enqs_supp_add2 enqs_supp_add3 enqs_pin_code | Our Requirements | Technical Delivery Condirions of Material
Test Certificate Y | AS PER SPECIFICATION NO. AA 51420 REV. 01 & ENQUIRY DESCRIPTION.
Guarantee Certificate N
Instruction Booklet N | Inspection Requirements
Sample Y | BY QC DEPTT., BHEL, BHOPAL.
Original Gate Pass Y

Sl No. | Material Code | Description& Specification | Unit | Quantity | Delivery Schedule
Lot No. | Quantity | Destin. | Date
1 | AA5141520013 | MULTILAYERED CROSS LAMINATED POLYETHYLENE FILM OF 45 GSM TO SIZE : 2440 MM WIDE X 50 METRE LONG PACKET IN NATURAL COLOUR (TO SPECIFICATION NO. AA 514 20 - REV. 01) WITH "BHEL" MONOGRAM ON EVERY ONE METRE LENGTH OF FILM. EACH PACKET TO BE MARKED WITH RED / BLUE INK AS "45 GSM". TWO VERTICAL HEAT SEALING JOINTS WILL BE ACCEPTABLE AT THE INTERVAL OF 1200 MM WIDTH PROVIDED TENSILE STRENGTH ACROSS HEAT SEALING JOINT IS AS PER CORPORATE PURCHASING SPECIFICATION : AA 51420 REV. 01. | NO | 500 |
1 | 250.000 | 881 | 15-10-08
2 | 250.000 | 881 | 31-12-08
2 | AA5141520030 | MULTILAYERED CROSS LAMINATED POLYETHYLENE FILM OF 70 GSM TO SIZE : 3660 MM WIDE X 50 METRE LONG PACKET IN YELLOW COLOUR (TO SPECIFICATION NO. AA 514 20 - REV. 01) WITH "BHEL" MONOGRAM ON EVERY ONE METRE LENGTH OF FILM. EACH PACKET TO BE MARKED WITH RED / BLUE INK AS "70 GSM". TWO VERTICAL HEAT SEALING JOINTS WILL BE ACCEPTABLE AT THE INTERVAL OF 1200 MM WIDTH PROVIDED TENSILE STRENGTH ACROSS HEAT SEALING JOINT IS AS PER CORPORATE PURCHASE SPECIFICATION : AA 514 20 REV. 01. | NO | 2000 |
1 | 1,000.000 | 881 | 31-01-09
2 | 1,000.000 | 881 | 15-04-09
3 | AA5141520040 | MULTILAYERED CROSS LAMINATED POLYETHYLENE FILM OF 90 GSM TO SIZE : 3660 MM WIDE X 50 METRE LONG PACKET IN NATURAL COLOUR WITH "BHEL" (MONOGRAM), "90 GSM - EXPORT" ON EVERY ONE METRE LENGTH OF FILM. TWO VERTICAL HEAT SEALING JOINTS WILL BE ACCEPTABLE AT THE INTERVAL OF 1200 MM WIDTH PROVIDED TENSILE STRENGTH ACROSS HEAT SEALING JOINT IS AS PER CORPORATE PURCHASING SPECIFICATION : AA 514 20 REV. 01. EACH FILM PACKET TO BE MARKED WITH RED / BLUE INK AS "90 GSM - EXPORT". | NO | 100 |
1 | 100.000 | 881 | 15-10-08

Dear Sir Please submit your lowest quotation for the above material subject to our terms & conditions enclosed so as to reach us on or before the due date by 11:00 A.M. Please note that: 1. This is only request for Quotation & not an Order. 2.Small Scale Industries should Indicate SSI Regn. No. in Quotation / Invoice. 3.In case you are not making an offer against this Enquiry , we request you to post a regret letter. | Remarks (1) OFFER SHOULD BE SUBMITTED IN TWO PART BID SYSTEM I.E. TECHNO-COMMERCIAL BID AS PART - I AND PRICE BID AS PART - II, SEPARATELY. (2) FOR DETAILS REFER ENQUIRY SHEET & ANNEXURE - 1 TO ANNEXURE - 8 ENCLOSED HEREWITH.
Documets Enclosed Drawing N Catalogue N Purchase Specification Y Quality Surveilliance Plan N | For and Behalf of BHEL SHRI A L VISHWAKARMA SR DGM(MM-MFS) 1232851 (Sign. / & Seal)